========================
      © LAN TO LAN
========================
  -----------------------------------------------------------------------------     
  User last login information:     
  -----------------------------------------------------------------------------
  Access Type: Telnet      
  IP-Address : 10.161.122.25     
  Time       : 2024-02-07 17:07:56+05:00     
  -----------------------------------------------------------------------------
<UNID_PC_UNQ9999_PPAL>
<UNID_PC_UNQ9999_PPAL>dis ip int brief
*down: administratively down
^down: standby
(l): loopback
(s): spoofing
(E): E-Trunk down
The number of interface that is UP in Physical is 5
The number of interface that is DOWN in Physical is 4
The number of interface that is UP in Protocol is 3
The number of interface that is DOWN in Protocol is 6

Interface                         IP Address/Mask      Physical   Protocol  
Cellular0/0/0                     unassigned           down       down      
Cellular0/0/1                     unassigned           down       down      
GigabitEthernet0/0/0              172.20.0.4/24        up         up        
GigabitEthernet0/0/1              unassigned           up         down      
GigabitEthernet0/0/1.2570         10.161.122.26/30     up         up        
GigabitEthernet0/0/2              192.168.1.1/24       down       down      
GigabitEthernet0/0/3              unassigned           up         down      
NULL0                             unassigned           up         up(s)     
Vlanif1                           unassigned           down       down      

<UNID_PC_UNQ9999_PPAL>
<UNID_PC_UNQ9999_PPAL>ping -a 172.20.0.4 172.16.30.1
  PING 172.16.30.1: 56  data bytes, press CTRL_C to break
    Reply from 172.16.30.1: bytes=56 Sequence=1 ttl=254 time=4 ms
    Reply from 172.16.30.1: bytes=56 Sequence=2 ttl=254 time=4 ms
    Reply from 172.16.30.1: bytes=56 Sequence=3 ttl=254 time=5 ms
    Reply from 172.16.30.1: bytes=56 Sequence=4 ttl=254 time=5 ms
    Reply from 172.16.30.1: bytes=56 Sequence=5 ttl=254 time=5 ms

  --- 172.16.30.1 ping statistics ---
    5 packet(s) transmitted
    5 packet(s) received
    0.00% packet loss
    round-trip min/avg/max = 4/4/5 ms

<UNID_PC_UNQ9999_PPAL>

<UNID_PC_UNQ9999_PPAL>ping -a 172.20.0.4  172.16.20.1 
  PING 172.16.20.1: 56  data bytes, press CTRL_C to break
    Reply from 172.16.20.1: bytes=56 Sequence=1 ttl=64 time=2 ms
    Reply from 172.16.20.1: bytes=56 Sequence=2 ttl=64 time=3 ms
    Reply from 172.16.20.1: bytes=56 Sequence=3 ttl=64 time=2 ms
    Reply from 172.16.20.1: bytes=56 Sequence=4 ttl=64 time=2 ms
    Reply from 172.16.20.1: bytes=56 Sequence=5 ttl=64 time=2 ms

  --- 172.16.20.1 ping statistics ---
    5 packet(s) transmitted
    5 packet(s) received
    0.00% packet loss
    round-trip min/avg/max = 2/2/3 ms

<UNID_PC_UNQ9999_PPAL>
